ICD-G0002

Telescope Tube Mass Balance F/16 Optical Top End

M. Sheehan

July 14, 1993

Approved by Systems Engineer: _____________________

GEMINI PROJECT OFFICE 950 N. Cherry Ave. Tucson, Arizona 85719 Phone: (520) 318-8545 Fax: (520) 318-8590

ICD-G0002

Revision Control Descriptions

Revision:

Date:

Approved:

Description:

ICD-G0002 Page 2 of 3

This General Interface Document defines the telescope tube mass balance for the f/16 optical top end configuration.

Subsystem Mass (kg) Center of Gravity (m) Static Moment (kg-m)

Xref Yref Zref X Y

Main Truss 7870.0 0.00 0.00 7.56 0.0 f/16 Top End 6067.6 0.00 0.00 13.69 0.0

Center Section 47167.5 0.00 0.00 -0.60 0.0

Primary Mirror Support Frame 22850.0 0.00 0.00 -1.73 0.0

Primary Mirror and Cell 69700.0 0.00 0.00 -0.49 0.0

Cassegrain Instruments 13000.0 0.00 0.00 -3.12 0.0

166655.1 0.00 0.00 0.00 0.0

ICD-G0002 Page